From 9012c6fb7c040be92aa8f950bad4f49c5be264d8 Mon Sep 17 00:00:00 2001
From: Amlal El Mahrouss <amlal@nekernel.org>
Date: Sun, 28 Dec 2025 09:23:05 +0100
Subject: feat! rename docs to doc.

Signed-off-by: Amlal El Mahrouss <amlal@nekernel.org>
---
 docs/tex/mini_bus_controller_interface.tex | 117 -----------------------------
 1 file changed, 117 deletions(-)
 delete mode 100644 docs/tex/mini_bus_controller_interface.tex

(limited to 'docs/tex/mini_bus_controller_interface.tex')

diff --git a/docs/tex/mini_bus_controller_interface.tex b/docs/tex/mini_bus_controller_interface.tex
deleted file mode 100644
index ba2381b7..00000000
--- a/docs/tex/mini_bus_controller_interface.tex
+++ /dev/null
@@ -1,117 +0,0 @@
-
-\documentclass{article}
-\usepackage{geometry}
-\usepackage{longtable}
-\usepackage{listings}
-\usepackage{xcolor}
-\geometry{margin=1in}
-\title{MBCI: Mini Bus Controller Interface Specification}
-\author{Amlal El Mahrouss}
-\date{\today}
-
-\begin{document}
-
-\maketitle
-
-\section{Overview}
-The Mini Bus Controller Interface (MBCI) is a standardized memory-mapped I/O bus specification designed for use in embedded systems and operating system kernels. It provides an extensible framework for managing hardware devices via a shared bus using memory-mapped registers. It is designed to remain abstract and platform-agnostic, leaving platform-specific interrupt and address logic to the HAL.
-
-\section{Signal Lines}
-The MBCI bus interface includes the following signal lines:
-
-\begin{itemize}
-  \item \textbf{VCC} (IN) – Power supply (OUT for MCU)
-  \item \textbf{CLK} (IN) – Clock line (OUT for MCU)
-  \item \textbf{ACK} (BI) – Acknowledge line containing packet frame
-  \item \textbf{D0-, D1-} (IN) – Host interface packet input
-  \item \textbf{D0+, D1+} (OUT) – Host interface packet output
-  \item \textbf{GND} (IN) – Ground line (OUT for MCU)
-\end{itemize}
-
-\section{Host Structure}
-
-\subsection*{IMBCIHost Structure}
-
-\begin{lstlisting}[language=C++,basicstyle=\ttfamily\footnotesize]
-volatile struct IMBCIHost {
-  UInt32 Magic;
-  UInt32 HostId;
-  UInt16 VendorId;
-  UInt16 DeviceId;
-  UInt8  MemoryType;
-  UInt16 HostType;
-  UInt16 HostFlags;
-  UInt8  Error;
-  UInt32 MMIOTest;
-  UInt16 State;
-  UInt8  Status;
-  UInt8  InterruptEnable;
-  UInt64 BaseAddressRegister;
-  UInt64 BaseAddressRegisterSize;
-  UInt32 CommandIssue;
-  UInt8  Esb[64];  // Extended Signature Block
-  UInt8  Zero[8];
-};
-\end{lstlisting}
-
-\section{Enumerations}
-
-\subsection*{Device Speeds}
-\begin{itemize}
-  \item \texttt{kMBCISpeedDeviceInvalid}
-  \item \texttt{kMBCILowSpeedDevice}
-  \item \texttt{kMBCIHighSpeedDevice}
-\end{itemize}
-
-\subsection*{Host Flags}
-\begin{itemize}
-  \item \texttt{kMBCIHostFlagsSupportsNothing}
-  \item \texttt{kMBCIHostFlagsSupportsAPM}
-  \item \texttt{kMBCIHostFlagsSupportsDaisyChain}
-  \item \texttt{kMBCIHostFlagsSupportsHWInterrupts}
-  \item \texttt{kMBCIHostFlagsSupportsDMA}
-  \item \texttt{kMBCIHostFlagsExtended}
-\end{itemize}
-
-\subsection*{Host Types}
-\begin{itemize}
-  \item \texttt{kMBCIHostKindHardDisk}
-  \item \texttt{kMBCIHostKindOpticalDisk}
-  \item \texttt{kMBCIHostKindKeyboardLow}
-  \item \texttt{kMBCIHostKindMouseLow}
-  \item \texttt{kMBCIHostKindMouseHigh}
-  \item \texttt{kMBCIHostKindKeyboardHigh}
-  \item \texttt{kMBCIHostKindNetworkInterface}
-  \item \texttt{kMBCIHostKindDaisyChain}
-  \item \texttt{kMBCIHostKindStartExtended}
-\end{itemize}
-
-\subsection*{Host State}
-\begin{itemize}
-  \item \texttt{kMBCIHostStateInvalid}
-  \item \texttt{kMBCIHostStateReset}
-  \item \texttt{kMBCIHostStateSuccess}
-  \item \texttt{kMBCIHostStateReady}
-  \item \texttt{kMBCIHostStateDmaStart}
-  \item \texttt{kMBCIHostStateDmaEnd}
-  \item \texttt{kMBCIHostStateFail}
-  \item \texttt{kMBCIHostStateCount}
-\end{itemize}
-
-\section{Functions}
-
-\subsection*{MMIO Test}
-Tests if MMIO is accessible by writing and checking a challenge value. Times out if the bus does not respond.
-
-\begin{lstlisting}[language=C++,basicstyle=\ttfamily\footnotesize]
-inline BOOL busi_test_mmio(struct IMBCIHost* host, const UInt32 test);
-\end{lstlisting}
-
-\subsection*{Auth Key Reader}
-Reads the 24-bit auth key encoded in the last three bytes of the Extended Signature Block after verifying MMIO test success:
-
-\begin{lstlisting}[language=C++,basicstyle=\ttfamily\footnotesize]
-inline MBCIAuthKeyType mbci_read_auth_key(struct IMBCIHost* host);
-\end{lstlisting}
-
-\end{document}
-- 
cgit v1.2.3

